**SIX MONTH SURVEILLANCE**

 **HOMOGENEOUS ACBM RECORDS** Date of Inspection:

District: Colusa Unified School District Inspector:

School: Egling Middle School Building: Administration

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| MaterialClass | Material | Homo. Mat. # | % Asb. | Ft2((S)/L.F.(L)  | Location  | Condition: Code & Comments | FriableYes/No |
| M | WALLBOARD & JOINT COMPOUND | 01 | ASSUMED | UNDETERMINED | THROUGHOUT BUILDING | (1) (4) | N |
| S | SKIM COAT | 02 | ASSUMED | 100 S | NURSE’S OFFICE AND RESTROOM AT CEILINGS | (1) (4)  | N |
| M | LIGHT TAN 12" VFT & MASTIC | 07 | ASSUMED | 145 S | MAIN OFFICE, COUNSELING OFFICE, NURSE’S ROOM & RESTROOM | (1) (4) | N |
| M | DARK TAN 12" VFT & MASTIC | 08 | ASSUMED | 240 S | ADMINISTRATIVE LOBBY | (1) (4) | N |
| M | CARPET GLUE | 12 | ASSUMED | 300 S | MAIN OFFICE, PRINCIPAL OFFICE AND VP OFFICE | (1) (4)  | N |
| M | 2X4 CEILING PANELS | 13 | ASSUMED | 600 S | MAIN OFFICE, PRINCIPAL OFFICE, VP OFFICE AND COUNSELING OFFICE | (1) (4)  | N |
| M | STUCCO | 001 | ASSUMED |  UNDETERMINED | EXTERIOR WALKWAYS THROUGHOUT SITE | (1) | N |
| M | A/C TRANSITE PANELS | 16 | ASSUMED | 140 S | OVER WINDOWS IN MEN’S & WOMEN’S RESTROOMS & EXTERIOR | (1) (4) | N |

 Z:\Clients\Colusa Unified School District\14-3310 3 Year Reinspections\Sites\Egling Middle School\Egling MS - HMR - 6 Month.wpd

CONDITION CODE

General Condition: (1) Good (2) Damaged (3) Significantly Damaged (25% or more)

Change in Condition: (4) No (5) Yes (If Yes, explain under comments)

Abated: (6) Repaired (7) Removed (8) Encapsulated (9) Enclosed (10) Isolated & Restricted

Miscellaneous: (11) Inaccessible, no inspection data (12) Other (Explain under comments) (13) Non-Asbestos/Not Inspected

 (14) Non AHERA/Not Inspected

**CONSULT ORIGINAL AND SUPPLEMENTARY INSPECTION REPORTS FOR MATERIALS WITH TRACE AMOUNTS OF ASBESTOS**

**SIX MONTH SURVEILLANCE**

 **HOMOGENEOUS ACBM RECORDS** Date of Inspection:

District: Colusa Unified School District Inspector:

School: Egling Middle School Building: Wing 100

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| MaterialClass | Material | Homo. Mat. # | % Asb. | Ft2/L.F.  | Location  | Condition: Code & Comments | FriableYes/No |
| M | WALLBOARD & JOINT COMPOUND | 01 | ASSUMED | UNDETERMINED | CENTER WORK STATIONS (3), RESTROOMS (4), SUPPLY ROOMS (3), CUSTODIAL ROOMS (2), & BOILER ROOM | (1) (4) | N |
| S | SKIM COAT | 03 | ASSUMED | 400 S | RESTROOMS (4) | (1) (4)  | N |
| M | 12" VINYL FLOOR TILE & MASTIC  | 09 | ASSUMED | 1,000 S | CENTER WORK STATIONS (3), SUPPLY ROOMS (3) AND CUSTODIAL ROOMS (2) | (1) (4) | N |
| M | 12" ACT & MASTIC | 14 | ASSUMED | 1,000 S | CENTER WORK STATIONS (3), SUPPLY ROOMS (3) AND CUSTODIAL ROOMS (2) | (1) (4) | N |
| M | CARPET GLUE | 12 | ASSUMED | 10,000 S | CLASSROOMS (12) AND MEDIA ROOM | (1) (4)  | N |
| M | 2X4 CEILING PANELS | 13 | ASSUMED | 10,000 S | CLASSROOMS (12) AND MEDIA ROOM | (1) (4)  | N |
| M | A/C TRANSITE PANELS | 16 | ASSUMED | 640 S | EXTERIOR - ABOVE & BELOW ALL WINDOWS AND DOORS (91 LOCATIONS) | (1) (4) | N |

Z:\Clients\Colusa Unified School District\14-3310 3 Year Reinspections\Sites\Egling Middle School\Egling MS - HMR - 6 Month.wpd

CONDITION CODE

General Condition: (1) Good (2) Damaged (3) Significantly Damaged (25% or more)

Change in Condition: (4) No (5) Yes (If Yes, explain under comments)

Abated: (6) Repaired (7) Removed (8) Encapsulated (9) Enclosed (10) Isolated & Restricted

Miscellaneous: (11) Inaccessible, no inspection data (12) Other (Explain under comments) (13) Non-Asbestos/Not Inspected

 (14) Non AHERA/Not Inspected

**CONSULT ORIGINAL AND SUPPLEMENTARY INSPECTION REPORTS FOR MATERIALS WITH TRACE AMOUNTS OF ASBESTOS**

**SIX MONTH SURVEILLANCE**

 **HOMOGENEOUS ACBM RECORDS** Date of Inspection:

District: Colusa Unified School District Inspector:

School: Egling Middle School Building: Wing 200

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| MaterialClass | Material | Homo. Mat. # | % Asb. | Ft2/L.F.  | Location  | Condition: Code & Comments | FriableYes/No |
| M | WALLBOARD & JOINT COMPOUND | 01 | ASSUMED | UNDETERMINED | RESTROOMS (2) | (1) (4)  | N |
| S | TEXTURE | 04 | ASSUMED | 100 S | GIRLS RESTROOM | (1) (4)  | N |
| S | ACOUSTIC TEXTURE | 05 | ASSUMED | 100 S | BOYS RESTROOM | (1) (4) | N |
| M | 12" VINYL FLOOR TILE (TAN) & MASTIC | 10 | ASSUMED | 2,260 S  | ROOMS 202-205, 210, 214, 222, PAINT ROOM, CUSTODIAL ROOM CHEMISTRY, STORE ROOM AND WORK ROOM  | (1) (4) | N |
| M | 12" VINYL FLOOR TILE (OFF WHITE) & MASTIC | 11 | ASSUMED | 500 S | ROOM 220 | (1) (4) | N |
| M | CARPET GLUE | 12 | ASSUMED | 10,000 S | CLASSROOMS (12) AND MEDIA ROOM | (1) (4)  | N |
| M | 2X4 CEILING PANELS | 13 | ASSUMED | 10,000 S | CLASSROOMS (12) AND MEDIA ROOM | (1) (4)  | N |
| T | PIPE ELBOWS (MUDDED) | 15 | ASSUMED | 6 EA. | CUSTODIAL CLOSET | (1) (4)  | Y |
| M | A/C TRANSITE PANELS | 16 | ASSUMED | 695 S | VENDING MACHINE AREA AND EXTERIOR OF BUILDING | (1) (4) | N |

 Z:\Clients\Colusa Unified School District\14-3310 3 Year Reinspections\Sites\Egling Middle School\Egling MS - HMR - 6 Month.wpd

CONDITION CODE

General Condition: (1) Good (2) Damaged (3) Significantly Damaged (25% or more)

Change in Condition: (4) No (5) Yes (If Yes, explain under comments)

Abated: (6) Repaired (7) Removed (8) Encapsulated (9) Enclosed (10) Isolated & Restricted

Miscellaneous: (11) Inaccessible, no inspection data (12) Other (Explain under comments) (13) Non-Asbestos/Not Inspected

 (14) Non AHERA/Not Inspected

**CONSULT ORIGINAL AND SUPPLEMENTARY INSPECTION REPORTS FOR MATERIALS WITH TRACE AMOUNTS OF ASBESTOS**

**SIX MONTH SURVEILLANCE**

 **HOMOGENEOUS ACBM RECORDS** Date of Inspection:

District: Colusa Unified School District Inspector:

School: Egling Middle School Building: Wing 400

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| MaterialClass | Material | Homo. Mat. # | % Asb. | Ft2/L.F.  | Location  | Condition: Code & Comments | FriableYes/No |
| M | WALLBOARD & JOINT COMPOUND | 01 | ASSUMED | UNDETERMINED | KITCHEN, DRY STORAGE ROOM, SPORTS STORAGE ROOM, AND COACH OFFICES (2) | (1) (4)  | N |
| S | TEXTURE | 06 | ASSUMED | 300 S | KITCHEN AND DRY STORAGE ROOM | (1) (4) | N |
| M | 12" VINYL FLOOR TILE (TAN) & MASTIC | 10 | ASSUMED | 2,400 S  | MULTI-PURPOSE ROOM | (1) (4) | N |
| M | 12" VINYL FLOOR TILE (OFF WHITE) & MASTIC | 11 | ASSUMED | 500 S | KITCHEN, DRY STORAGE ROOM, ANC COACH OFFICES (2) | (1) (4) | N |
| M | 2X4 CEILING PANELS | 13 | ASSUMED | 2,400 S | MULTI-PURPOSE ROOM | (1) (4)  | N |
| M | 12" ACT & MASTIC | 14 | ASSUMED | 3,840 S | GYM | (1) (4)  | N |
| M | A/C TRANSITE PANELS | 16 | ASSUMED | 695 S | WEST EXTERIOR OF BUILDING | (1) (4) | N |

 Z:\Clients\Colusa Unified School District\14-3310 3 Year Reinspections\Sites\Egling Middle School\Egling MS - HMR - 6 Month.wpd

CONDITION CODE

General Condition: (1) Good (2) Damaged (3) Significantly Damaged (25% or more)

Change in Condition: (4) No (5) Yes (If Yes, explain under comments)

Abated: (6) Repaired (7) Removed (8) Encapsulated (9) Enclosed (10) Isolated & Restricted

Miscellaneous: (11) Inaccessible, no inspection data (12) Other (Explain under comments) (13) Non-Asbestos/Not Inspected

 (14) Non AHERA/Not Inspected

**CONSULT ORIGINAL AND SUPPLEMENTARY INSPECTION REPORTS FOR MATERIALS WITH TRACE AMOUNTS OF ASBESTOS**

**SIX MONTH SURVEILLANCE**

 **HOMOGENEOUS ACBM RECORDS** Date of Inspection:

District: Colusa Unified School District Inspector:

School: Egling Middle School Building: Band

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| MaterialClass | Material | Homo. Mat. # | % Asb. | Ft2/L.F.  | Location  | Condition: Code & Comments | FriableYes/No |
| M | 12" ACT & MASTIC | 17 | ASSUMED | 1,200 S | BAND ROOM | (1) (4) | N |
| M | WINDOW PUTTY | 18 | ASSUMED | THROUGHOUT | BAND ROOM | (1) (4) | N |

 Z:\Clients\Colusa Unified School District\14-3310 3 Year Reinspections\Sites\Egling Middle School\Egling MS - HMR - 6 Month.wpd

CONDITION CODE

General Condition: (1) Good (2) Damaged (3) Significantly Damaged (25% or more)

Change in Condition: (4) No (5) Yes (If Yes, explain under comments)

Abated: (6) Repaired (7) Removed (8) Encapsulated (9) Enclosed (10) Isolated & Restricted

Miscellaneous: (11) Inaccessible, no inspection data (12) Other (Explain under comments) (13) Non-Asbestos/Not Inspected

 (14) Non AHERA/Not Inspected

**CONSULT ORIGINAL AND SUPPLEMENTARY INSPECTION REPORTS FOR MATERIALS WITH TRACE AMOUNTS OF ASBESTOS**